GUI Instructions for Dorna:

1. Run dorna\_gui\_v2 (This will automatically connect the robot)

2. Home robot joints

3. If robot not calibrated, move robot to zeros position, move non-calibrated joint to its zero position, then calibrate all joints

4. Before disconnecting, return robot to reset position